{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["实验室装修","基础化学实验室仪器","药物制剂实训室仪器","耗材"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"实验室装修","index":0,"n_rows":58,"n_cols":8,"rows_kept":58,"merged":[[0,0,0,7],[2,0,2,2],[17,0,17,4],[18,0,18,2],[30,0,30,4],[31,0,31,2],[44,0,44,4],[45,0,45,2],[56,0,56,4],[57,0,57,4]],"flags":["formulas_cached_only"]}
["实验台及装修报价"]
["序号","产品名称","产品规格（mm）","数量","单位","单价","金额","材质说明"]
["基础化学实验室"]
[1,"讲台","1600*700*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[2,"中央台","7500*1500*850",2,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[3,"边台","10200*750*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[4,"龙头水槽",null,4,"套",null,null,"实验室专用黑色PP水槽+三联化验水嘴"]
[5,"滴水架",null,4,"套",null,null,"整体实芯理化板+PP滴水棒+倒流管"]
[6,"单口洗眼器",null,2,"套",null,null,"整体采用铜制，表面喷涂环氧树脂涂层，喷头采用优质PP材质"]
[7,"龙头杯槽",null,11,"套",null,null,"实验室专用黑色双边PP杯槽+双边化验水嘴"]
[8,"试剂架",null,12.8,"m",null,null,"铝合金边框，10mm透明玻璃，吊线槽"]
[9,"实验凳",null,44,"张",null,null,"玻璃钢凳面，升降气杆结构"]
[10,"线盒插座",null,10,"套",null,null,"实验室专用单边斜面插座盒子+多功能插座"]
[11,"玻璃隔墙移位",null,25,"㎡",null,null,"旧有玻璃隔墙拆装，修复损坏部分"]
[12,"玻璃门移位",null,1,"樘",null,null,"旧有玻璃门拆装，修复损坏部分"]
[13,"钢化玻璃",null,1,"樘",null,null,"原有门洞钢化玻璃修复"]
[14,"水电改造",null,96,"㎡",null,null,"新益源国标电缆、台亚管道"]
["小计："]
["准备室"]
[1,"边台","6710*750*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[2,"转角柜","1000*1000*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[3,"边台","3215*750*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[4,"龙头水槽",null,1,"套",null,null,"实验室专用黑色PP水槽+三联化验水嘴"]
[5,"滴水架",null,1,"套",null,null,"整体实芯理化板+PP滴水棒+倒流管"]
[6,"单口洗眼器",null,1,"套",null,null,"整体采用铜制，表面喷涂环氧树脂涂层，喷头采用优质PP材质"]
[7,"器皿柜","900*420*1800",1,"座",null,null,"铝木结构，柜体采用E1级中纤板制作，上下门板、上门板带可视窗"]
[8,"药品柜","900*420*1800",1,"座",null,null,"铝木结构，柜体采用E1级中纤板制作，上下门板、上门板带可视窗"]
[9,"通风柜","1500*800*2350",2,"座",null,null,"全钢结构，标准上下柜，直排通风系统"]
[10,"线盒插座",null,10,"套",null,null,"实验室专用单边斜面插座盒子+多功能插座"]
[11,"水电改造",null,{"v":34.5,"d":"35"},"㎡",null,null,"新益源国标电缆、台亚管道"]
["小计："]
["药物制剂实训室"]
[1,"讲台","1600*700*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[2,"中央台","7500*1500*850",2,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[3,"边台","3500*750*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[4,"边台","4288*750*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[5,"边台","3813*750*850",1,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢"]
[6,"龙头水槽",null,4,"套",null,null,"实验室专用黑色PP水槽+三联化验水嘴"]
[7,"滴水架",null,4,"套",null,null,"整体实芯理化板+PP滴水棒+倒流管"]
[8,"单口洗眼器",null,4,"套",null,null,"整体采用铜制，表面喷涂环氧树脂涂层，喷头采用优质PP材质"]
[9,"试剂架",null,12.8,"m",null,null,"铝合金边框，10mm透明玻璃，吊线槽"]
[10,"实验凳",null,44,"张",null,null,"玻璃钢凳面，升降气杆结构"]
[11,"线盒插座",null,12,"套",null,null,"实验室专用单边斜面插座盒子+多功能插座"]
[10,"水电改造",null,100,"㎡",null,null,"新益源国标电缆、台亚管道"]
["小计："]
["药品室"]
[1,"药品柜","900*420*1800",20,"座",null,null,"铝木结构，柜体采用E1级中纤板制作，上下门板、上门板带可视窗"]
[2,"天平台","900*600*850",3,"座",null,null,"钢木结构：黑色实芯理化板台面+中纤板+40*60方钢+大理石减震块"]
[3,"货架","2000*600*1800",6,"座",null,null,"GB"]
[4,"危化品柜","1060*460*1650",3,"座",null,null,"双层结构，机械锁"]
[5,"酸碱柜","900*450*1800",3,"座",null,null,"耐腐蚀PP材质，双人双锁"]
[6,"防爆排气扇",null,2,"套",null,null,"GB"]
[7,"新建药品室隔墙",null,22,"㎡",null,null,"实心砖隔墙"]
[8,"钢质门",null,1,"樘",null,null,"GB"]
[9,"新建实体墙刷白",null,44,"㎡",null,null,"立邦涂料。\n批刮腻子两边，打磨平整后底漆面漆各一遍。"]
[10,"水电改造",null,64,"㎡",null,null,"新益源国标电缆、台亚管道"]
["小计："]
["合计："]

{"sheet":"基础化学实验室仪器","index":1,"n_rows":23,"n_cols":8,"rows_kept":23,"merged":[[0,0,0,7],[8,0,10,0],[8,1,10,1],[22,0,22,3]],"flags":["formulas_cached_only"]}
["基础化学实验室仪器报价"]
["序号","产品名称","产品规格/型号（mm）","数量","单位","单价","总价","品牌"]
[1,"电导率仪","DDSJ-308F",10,"台",null,null,"雷磁"]
[2,"电炉","1KW（单联）",10,"台",null,null,"慧泰"]
[3,"紫外分光光度计","UV-5100",6,"台",null,null,"元析"]
[4,"旋光测定仪","WZZ-2B",2,"台",null,null,"仪电物光"]
[5,"熔点仪","WRS-2",2,"台",null,null,"仪电物光"]
[6,"PH计","PHS-3C",10,"台",null,null,"雷磁"]
[1,"数显恒温电热套","DRT-SX 500ml数显",10,"台",null,null,"长城科工贸"]
[null,null,"DRT-SX 3000ml数显",10,"台",null,null,"长城科工贸"]
[null,null,"DRT-SX 5000ml数显",10,"台",null,null,"长城科工贸"]
[2,"旋转蒸发仪","R-1001VN",5,"台",null,null,"长城科工贸"]
[3,"旋转蒸发仪","R-3001",5,"台",null,null,"长城科工贸"]
[4,"水浴锅","HH-2",2,"台",null,null,"常州国华"]
[5,"真空泵","SHB-III",2,"台",null,null,"长城工贸"]
[6,"电吹风","FH6218",2,"台",null,null,"飞科"]
[7,"离心机","L3-5k（配6*50角转子）",2,"台",null,null,"可成"]
[8,"磁力搅拌器","78--1",5,"台",null,null,"常州国华"]
[9,"真空干燥箱","DZF-6050（含泵）",2,"台",null,null,"上海新苗"]
[10,"超声波清洗器","KQ-250E",2,"台",null,null,"昆山舒美"]
[1,"电子天平","FA2004B ",7,"台",null,null,"佑科"]
[3,"显微镜","BM1800",10,"台",null,null,"江南永新"]
["小计："]

{"sheet":"药物制剂实训室仪器","index":2,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[0,0,0,7],[26,0,26,3]],"flags":["formulas_cached_only"]}
["药物制剂实训室仪器报价"]
[1,"胶囊填充板","0#;1#;2#;3#",5,"台",null,null,"/"]
[2,"溶出仪","ZRS-1",5,"台",null,null,"欧莱博"]
[3,"崩解仪","BJ-1",5,"台",null,null,"欧莱博"]
[4,"硬度仪","YD-1",5,"台",null,null,"欧莱博"]
[5,"筛网","20目/40目/60目/80目/100目/120目",5,"台",null,null,"/"]
[6,"摇摆式的湿法制粒机","YK-60",2,"台",null,null,"国卫和教"]
[7,"混合仪","WCH-10",2,"台",null,null,"国卫和教"]
[8,"包衣机","B300D",1,"台",null,null,"国卫和教"]
[9,"旋转式压片机","ZP-9D",2,"台",null,null,"国卫和教"]
[10,"超微粉碎机","XL-30C",2,"台",null,null,"欧莱博"]
[11,"小型粉碎机","XL-06A",5,"台",null,null,"欧莱博"]
[12,"脆翠度检查仪","CS-1",2,"台",null,null,"欧莱博"]
[14,"普通冰箱","YCD-265",1,"台",null,null,"奥柯玛"]
[15,"熔封机","ARF",5,"台",null,null,"国卫和教"]
[16,"澄明度检查装置","CM-1",5,"台",null,null,"欧莱博"]
[17,"高压灭菌器","BKQ-B50II",5,"台",null,null,"博科"]
[18,"煎煮锅","OLB20-1+1（70-260）",5,"台",null,null,"欧莱博"]
[19,"滴丸机","DLC-6",1,"台",null,null,"国卫和教"]
[20,"单冲压片机","TDP-5",2,"台",null,null,"国卫和教"]
[21,"自动双重纯水蒸馏器","SZ-93",5,"台",null,null,"上海亚荣"]
[22,"四用仪","ZPJ-4",5,"台",null,null,"欧莱博"]
[23,"四管崩解仪","BJ-4",5,"台",null,null,"欧莱博"]
[24,"碎度检查仪","CS-4 ",5,"台",null,null,"欧莱博"]
[25,"真空冷冻干燥机","OLB-FD10S",2,"台",null,null,"欧莱博"]
[26,"小型空压机",null,2,"台",null,null,"/"]
["小计："]

{"sheet":"耗材","index":3,"n_rows":190,"n_cols":9,"rows_kept":190,"merged":[[189,0,189,3]],"flags":["formulas_cached_only"]}
[1,"精密PH试纸"," 1-14.",200,"盒",null,null,"GB"]
[2,"玻璃电极","E-201F",20,"个",null,null,"GB","雷磁"]
[3,"717强碱性阴离子交换树脂","A854519-250g",20,"个",null,null,"GB","麦克林"]
[4,"732强酸性阳离子交换树脂","A821221-500g",20,"个",null,null,"GB","麦克林"]
[5,"酒精喷灯",null,5,"个",null,null,"GB","铜酒精喷灯坐式"]
[6,"安瓿割颈器",null,50,"个",null,null,"GB"]
[7,"垂熔玻璃滤器",null,50,"个",null,null,"GB","50ML G1-G5选择规格"]
[8,"灌注器",null,50,"支",null,null,"GB","灌注器 250Ml"]
[9,"微孔滤膜（0.8μm）","50MM直径水系",50,"盒",null,null,"GB","50张/盒 兴亚"]
[10,"薄层板","25*50",50,"盒",null,null,"GB","一盒320片"]
[11,"薄层色谱展开缸","100*100双槽",50,"个",null,null,"GB","层析缸P-1"]
[12,"变色喷雾瓶",null,50,"组",null,null,"GB","显色喷雾瓶"]
[13,"刻度试管","1-5ML",80,"个",null,null,"GB","5ML"]
[14,"无刻度试管","胖肚1-5ML",80,"个",null,null,"GB","胖肚吸管5ML 齿轮"]
[15,"离心试管","5ML，300支/包",80,"包",null,null,"GB","塑料压盖圆底离心管 300支/包"]
[16,"具塞刻度试管","10ML",80,"个",null,null,"GB"]
[17,"具塞试管","25ML刻度 ",80,"个",null,null,"GB"]
[18,"烧杯","3000ml ",80,"个",null,null,"GB"]
[19,"烧杯"," 1000ml ",80,"个",null,null,"GB"]
[20,"烧杯"," 500ml ",80,"个",null,null,"GB"]
[21,"烧杯"," 250ml ",80,"个",null,null,"GB"]
[22,"烧杯"," 50ml",80,"个",null,null,"GB"]
[23,"碘量瓶","250ML",80,"个",null,null,"GB"]
[24,"碘量瓶","500ML",80,"个",null,null,"GB"]
[25,"锥型瓶","100ml",80,"个",null,null,"GB"]
[26,"锥型瓶","250ml",80,"个",null,null,"GB"]
[27,"锥型瓶","500ml",80,"个",null,null,"GB"]
[28,"锥型瓶","1000ml",80,"个",null,null,"GB"]
[29,"容量瓶","1000ml ",80,"个",null,null,"GB"]
[30,"容量瓶"," 500ml ",80,"个",null,null,"GB"]
[31,"容量瓶"," 250ml ",80,"个",null,null,"GB"]
[32,"容量瓶"," 100ml ",80,"个",null,null,"GB"]
[33,"容量瓶"," 50ml ",80,"个",null,null,"GB"]
[34,"容量瓶"," 25ml ",80,"个",null,null,"GB"]
[35,"容量瓶"," 10ml ",80,"个",null,null,"GB"]
[36,"圆底烧瓶","100ML/24",80,"个",null,null,"GB"]
[37,"圆底烧瓶","250ML/24",80,"个",null,null,"GB"]
[38,"圆底烧瓶","500ML/24",80,"个",null,null,"GB"]
[39,"圆底烧瓶","1000ML/24",80,"个",null,null,"GB"]
[40,"平底烧瓶","100ML/24",80,"个",null,null,"GB"]
[41,"平底烧瓶","250ML/24",80,"个",null,null,"GB"]
[42,"平底烧瓶","500ML/24",80,"个",null,null,"GB"]
[43,"平底烧瓶","1000ML/24",80,"个",null,null,"GB"]
[44,"二口烧瓶","250ML/24",80,"个",null,null,"GB","确定是直口还是斜口"]
[45,"二口烧瓶","500ML/24",80,"个",null,null,"GB","确定是直口还是斜口"]
[46,"二口烧瓶","1000ML/24",80,"个",null,null,"GB","确定是直口还是斜口"]
[47,"三口烧瓶","250ML/24",80,"个",null,null,"GB","确定是直口还是斜口"]
[48,"三口烧瓶","500ML/24",80,"个",null,null,"GB","确定是直口还是斜口"]
[49,"三口烧瓶","1000ML/24",80,"个",null,null,"GB","确定是直口还是斜口"]
[50,"四口烧瓶","250ML/24",80,"个",null,null,"GB","直口还是斜口"]
[51,"四口烧瓶","500ML/24",80,"个",null,null,"GB","直口还是斜口"]
[52,"四口烧瓶","1000ML/24",80,"个",null,null,"GB","直口还是斜口"]
[53,"蒸馏（支管）烧瓶","125ML",80,"个",null,null,"GB","具支蒸馏烧瓶 100ML 如图"]
[54,"蒸馏（支管）烧瓶","250ML",80,"个",null,null,"GB","具支蒸馏烧瓶 如图 仕富"]
[55,"蒸馏（支管）烧瓶","500ML",80,"个",null,null,"GB","具支蒸馏烧瓶 如图 仕富"]
[56,"分馏（凯式）烧瓶","100ML",80,"个",null,null,"GB","定氮凯氏烧瓶 如图"]
[57,"分馏（凯式）烧瓶","250ML",80,"个",null,null,"GB","定氮凯氏烧瓶 如图"]
[58,"分馏（凯式）烧瓶","500ML",80,"个",null,null,"GB","定氮凯氏烧瓶 如图"]
[59,"定氮烧瓶","100ML",80,"个",null,null,"GB","定氮凯氏烧瓶 如图"]
[60,"定氮烧瓶","250ML",80,"个",null,null,"GB","定氮凯氏烧瓶 如图"]
[61,"定氮烧瓶","500ML",80,"个",null,null,"GB","定氮凯氏烧瓶 如图"]
[62,"曲颈瓶","125ML",80,"个",null,null,"GB","仕富  如图"]
[63,"曲颈瓶","250ML",80,"个",null,null,"GB","仕富  如图"]
[64,"曲颈瓶","500ML",80,"个",null,null,"GB","仕富  如图"]
[65,"量筒","500ml",80,"个",null,null,"GB"]
[66,"量筒","250ml",80,"个",null,null,"GB"]
[67,"量筒","100ml",80,"个",null,null,"GB"]
[68,"量筒","50ml",80,"个",null,null,"GB"]
[69,"量杯","500ml",80,"个",null,null,"GB"]
[70,"量杯","1000ml ",80,"个",null,null,"GB"]
[71,"吸管","1ml  刻度",80,"个",null,null,"GB","刻度吸管"]
[72,"吸管","2ml 刻度",80,"个",null,null,"GB","刻度吸管"]
[73,"吸管","0.1ml 刻度",80,"个",null,null,"GB","刻度吸管"]
[74,"吸管","0.2ml 刻度",80,"个",null,null,"GB","刻度吸管"]
[75,"吸管","0.5ml 刻度",80,"个",null,null,"GB","刻度吸管"]
[76,"吸管","5ml 刻度",80,"个",null,null,"GB","刻度吸管"]
[77,"吸管","10ml 刻度",80,"个",null,null,"GB","刻度吸管"]
[78,"吸球","大",80,"个",null,null,"GB","洗耳球"]
[79,"吸球","中 ",80,"个",null,null,"GB","洗耳球"]
[80,"吸球","小 ",80,"个",null,null,"GB","洗耳球"]
[81,"移液管","1ml",20,"个",null,null,"GB","胖肚吸管"]
[82,"移液管","2ml",20,"个",null,null,"GB","胖肚吸管"]
[83,"移液管","3ml",20,"个",null,null,"GB","胖肚吸管"]
[84,"移液管","5ml",20,"个",null,null,"GB","胖肚吸管"]
[85,"移液管","10ml",20,"个",null,null,"GB","胖肚吸管"]
[86,"玻璃棒","中号",80,"个",null,null,"GB","7-8号"]
[87,"层析槽","层析缸P-1",50,"个",null,null,"GB","100*100"]
[88,"分液漏斗","100ml",80,"个",null,null,"GB","梨形分液漏斗125ML"]
[89,"分液漏斗"," 50ml ",null,"个",null,null,"GB","梨形分液漏斗60ML"]
[90,"试管架","4×10孔",50,"个",null,null,"GB","需要规格"]
[91,"研钵","8CM",50,"个",null,null,"GB","瓷研钵"]
[92,"研钵","10CM",50,"个",null,null,"GB","瓷研钵"]
[93,"研钵","16CM",50,"个",null,null,"GB","瓷研钵"]
[94,"蒸发皿","250ml",50,"个",null,null,"GB","瓷蒸发皿"]
[95,"蒸发皿"," 100ml ",50,"个",null,null,"GB","瓷蒸发皿"]
[96,"蒸发皿","50ml",50,"个",null,null,"GB","60ML 瓷蒸发皿"]
[97,"试剂瓶","无色250ML",80,"个",null,null,"GB","白大口 250ML"]
[98,"试剂瓶","无色500ML",80,"个",null,null,"GB","白大口瓶"]
[99,"试剂瓶","棕色250ML",80,"个",null,null,"GB","棕大口瓶"]
[100,"试剂瓶","棕色500ML",80,"个",null,null,"GB","棕大口瓶"]
[101,"布氏漏斗","200ml ",50,"个",null,null,"GB","200MM"]
[102,"布氏漏斗"," 150ml ",50,"个",null,null,"GB","150MM"]
[103,"布氏漏斗"," 100ml ",50,"个",null,null,"GB","100MM"]
[104,"布氏漏斗"," 50ml",50,"个",null,null,"GB","60MM "]
[105,"冷凝管","球200/24*2",50,"个",null,null,"GB"]
[106,"冷凝管","球300/24*2",50,"个",null,null,"GB"]
[107,"乳胶管","φ3mm～φ4mm/条",100,"米",null,null,"GB","4*6"]
[108,"抽滤瓶","500ml",50,"个",null,null,"GB","上嘴过滤瓶"]
[109,"抽滤瓶","1000ml",50,"个",null,null,"GB","上嘴过滤瓶"]
[110,"层析柱","10*150",30,"个",null,null,"GB","具塞层析柱"]
[111,"层析柱","10*200",30,"个",null,null,"GB","具塞层析柱"]
[112,"漏斗","75mm",80,"个",null,null,"GB","玻璃短管漏斗"]
[113,"漏斗","90mm ",80,"个",null,null,"GB","玻璃短管漏斗"]
[114,"干湿温度计","HTC-1",50,"个",null,null,"GB","数显温温度计"]
[115,"玻璃毛细管","0.9-1.1*100 熔点毛细管(0封)",30,"个",null,null,"GB","熔点毛细管(0封)"]
[116,"过滤瓶","250ml",50,"个",null,null,"GB","上嘴过滤瓶"]
[117,"过滤瓶","500ml",50,"个",null,null,"GB","上嘴过滤瓶"]
[118,"干燥器","210mm",10,"个",null,null,"GB"]
[119,"干燥器","240mm",10,"个",null,null,"GB"]
[120,"滴定管","酸式 25ml",50,"个",null,null,"GB"]
[121,"滴定管","酸式50ml",50,"个",null,null,"GB"]
[122,"滴定管"," 碱式25ml",50,"个",null,null,"GB"]
[123,"滴定管"," 碱式50ml",50,"个",null,null,"GB"]
[124,"胖肚移液管",null,50,"个",null,null,"GB","胖肚吸管没规格"]
[125,"移液管",null,50,"个",null,null,"GB","胖肚吸管没规格"]
[126,"胶头滴管","100MM",100,"个",null,null,"GB"]
[127,"滤纸","11CM",100,"盒",null,null,"GB","定量还是定性"]
[128,"滤纸","12.5CM",100,"盒",null,null,"GB","定量还是定性"]
[129,"冲洗瓶","红头250ml",50,"个",null,null,"GB","红头洗瓶"]
[130,"冲洗瓶","红头500ml",50,"个",null,null,"GB","红头洗瓶"]
[131,"喷壶","500ML",10,"个",null,null,"GB"]
[132,"酒精灯","250ML",50,"个",null,null,"GB"]
[133,"抽气管",null,30,"个",null,null,"GB","不知道什么"]
[134,"坩埚","30ML",50,"个",null,null,"GB","瓷坩埚"]
[135,"坩埚","50ML",50,"个",null,null,"GB","瓷坩埚"]
[136,"塑料桶",25,10,"个",null,null,"GB","25L塑料桶方桶"]
[137,"三脚架",null,50,"个",null,null,"GB"]
[138,"漏斗架","木制梨形漏斗架4孔开口",50,"个",null,null,"GB","木制 4孔/125-250ml"]
[139,"滴定夹","铁",80,"个",null,null,"GB","蝴蝶夹"]
[140,"镊子","16CM",80,"个",null,null,"GB","敷料镊"]
[141,"试管夹",null,80,"个",null,null,"GB","木试管夹"]
[142,"止水皮管夹",null,50,"个",null,null,"GB","弹簧止水夹"]
[143,"石棉网","20*20",80,"个",null,null,"GB"]
[144,"燃烧匙",null,50,"个",null,null,"GB","燃烧匙燃烧勺21cm"]
[145,"药匙","16CM",80,"个",null,null,"GB","不锈钢药勺"]
[146,"试管刷","大 ",50,"个",null,null,"GB"]
[147,"试管刷","中  ",50,"个",null,null,"GB"]
[148,"试管刷","小",50,"个",null,null,"GB"]
[149,"烧瓶刷","大 ",50,"个",null,null,"GB","三角烧瓶刷"]
[150,"烧瓶刷","中  ",50,"个",null,null,"GB","三角烧瓶刷"]
[151,"烧瓶刷","小",50,"个",null,null,"GB","三角烧瓶刷"]
[152,"坩埚钳","20CM",50,"个",null,null,"GB"]
[153,"坩埚钳","30CM",50,"个",null,null,"GB"]
[154,"表面皿","60mm",50,"个",null,null,"GB"]
[155,"表面皿","90mm",50,"个",null,null,"GB"]
[156,"表面皿","120mm",50,"个",null,null,"GB"]
[157,"载玻片",7101,400,"个",null,null,"GB"]
[158,"盖玻片","20*20",400,"个",null,null,"GB","100片/盒"]
[159,"白口瓶","250ML 塑料",80,"个",null,null,"GB"]
[160,"白口瓶","500ml 塑料",80,"个",null,null,"GB"]
[161,"称量瓶","50/30mm",80,"个",null,null,"GB"]
[162,"称量瓶","60/30mm",80,"个",null,null,"GB"]
[163,"称量瓶","70/35mm",80,"个",null,null,"GB"]
[164,"比色管"," 25ml",80,"个",null,null,"GB","具塞比色管"]
[165,"比色管"," 50ml",80,"个",null,null,"GB","具塞比色管"]
[166,"尾接管",null,50,"个",null,null,"GB","要图片"]
[167,"点样毛细管","0.3-100",80,"个",null,null,"GB","1000支/筒 按筒订"]
[168,"显色剂喷瓶","50ml",80,"个",null,null,"GB"]
[169,"色谱专用滤纸",null,20,"盒",null,null,"GB","请提供规格或品牌"]
[170,"聚酰胺色谱膜","10cm*10cm",20,"盒",null,null,"GB","一包50张 兴亚"]
[171,"表面皿","90mm",80,"个",null,null,"GB"]
[172,"表面皿","100mm",80,"个",null,null,"GB"]
[173,"表面皿","120mm",80,"个",null,null,"GB"]
[174,"投药瓶",null,80,"个",null,null,"GB"]
[175,"瓶签",null,80,"包",null,null,"GB","不清楚，最好提供图片"]
[176,"瓶塞",null,80,"盒",null,null,"GB","什么塞尺寸？"]
[177,"砂浴",null,5,"台",null,null,"GB","不知道什么"]
[178,"包药纸",null,20,"盒",null,null,"GB","4000张/包"]
[179,"带刻度有塞比浊管",null,80,"个",null,null,"GB","要图片"]
[180,"座标纸",null,20,"盒",null,null,"GB","什么规格A0/1/2/3/41"]
[181,"钢精锅",null,20,"个",null,null,"GB","不清楚"]
[182,"安瓿","2ml 910/盒",10,"盒",null,null,"GB","900支/盒"]
[183,"安瓿","5ml  230/盒",10,"盒",null,null,"GB","418支/盒"]
[184,"安瓿","10ml  300/盒",10,"盒",null,null,"GB","304支/盒"]
[185,"安瓿","20ml  210/盒",10,"盒",null,null,"GB","210支/盒"]
[186,"紫外灯",null,50,"把",null,null,"GB","格美斯紫外线消毒灯6W 有臭氧"]
[187,"不锈钢筛(20目和40目)",null,80,"套",null,null,"GB","手工不锈钢 20/40"]
[188,"药筛","200目内",50,"个",null,null,"GB","镀铬冲框"]
[189,"胶囊填充板",null,50,"块",null,null,"GB","0号 100孔"]
["小计："]